DMD, DMD Mounting, and Socket/Interposer Information Updated: 4 April 2026

Mounting Concept for Series 322 DMD
This mounting information provides a reference concept for mounting the DLP390TP 4K, DLP3951A-Q1, DLP3952A-Q1, and DLP3954A-Q1 0.39 DMDs. The DLP390TP DMD utilizes the FQZ package, DLP3951A-Q1, DLP3952A-Q1, and DLP3954A-Q1 utilize the FSD package. This mounting concept is for all Series 322 DMDs. Information includes: DMD 3D-CAD geometry model (STEP format) Link to DMD mechanical drawing - located at end of DMD data sheet Link to DMD data sheet (contains information like) Mounting and thermal load specifications Thermal specifications Array temperature calculation Electrical interconnect - mating connector information along with suppliers known at time of publishing Mechanical mounting concepts - has drawings (pdf format) and 3D-CAD geometry model (STEP format) for parts and assembly Getting Started Easy access to the files is provided with a web browser interface. Use of the web interface requires the files be downloaded and extracted to the computer. To utilize the web interface: Open the file 'READ-ME-s322-Mounting.htm' (this file) 'Right Click' on the downloaded file name and select ' Extract All...' (Note: Picking the file name will open the file but not extract the files) Select a destination to extract the files and select 'Extract' After extracting pick this link REVIEW_START-Series322.html or image below to start review (If the above link does not open the file or an image does not display below repeat Step (1) to extract the files)