Title: Bluetooth tester application

Description:

Tester application uses binary protocol to control Mynewt Nimble stack
and is aimed at automated testing. It uses Bluetooth Testing Protocol (BTP)
to drive Bluetooth stack. BTP commands and events are received and buffered for
further processing.
--------------------------------------------------------------------------------
Supported Profiles:

GAP, GATT, SM, L2CAP, MESH
--------------------------------------------------------------------------------

