CC33XX API Documentation 2.30.00.15

Public Attributes | List of all members
__PACKED__ Struct Reference
upper MAC

## Public Attributes
uint8_t | enableVal
uint8_t | padding [3]
uint8_t | index
uint32_t | value
uint8_t | rateVal
uint8_t | value
uint8_t | beaconRssi
uint8_t | overEnable
uint8_t | bw
uint8_t | preamble
uint8_t | rate
uint8_t | dcm
uint8_t | txPower
uint8_t | giLTF
uint32_t | receivedTotalPacketsNumber
uint32_t | receivedFcsErrorPacketsNumber
uint32_t | receivedAddressMismatchPacketsNumber
uint32_t | receivedGoodPackets
int16_t | averageDataCtrlRssi
int16_t | averageDataCtrlSNR
uint8_t | channel
uint8_t | band
uint8_t | bandwidth
uint32_t | bitmask
uint8_t | preambleType
uint8_t | phyRate
int8_t | txPower
uint8_t | GI_LTF_Type
uint8_t | DCM
uint16_t | startLength
uint16_t | endLength
uint32_t | delay
uint8_t | packetMode
uint16_t | numberOfPackets
uint8_t | dataMode
uint8_t | dataConstValue
uint8_t | enableCCA
uint8_t | bssColor
uint16_t | SU_ER_Bandwidth
uint8_t | partialAID
uint8_t | srcAddr [(6)]
uint8_t | dstAddr [(6)]
uint8_t | nominalPacketExtension
uint8_t | feedbackStatus
uint16_t | aid
uint8_t | groupId
uint8_t | ltfMode
uint8_t | heLtfNum
uint8_t | preFecPaddingFactor
uint16_t | commonInfoLen
uint16_t | ruAlloc
uint8_t | ulBw
uint8_t | startsStsNum
uint8_t | tbAutoMode
uint8_t | disamb
uint8_t | mode
int8_t | offset
int8_t | output_power
uint16_t | io_id
uint8_t | direction
uint8_t | state
uint8_t | ackEnable
uint8_t | macAddress [(6)]
uint8 | role_id
uint8 | pad [3]
uint32 | missed_beacons
uint8 | snr_data
uint8 | snr_beacon
int8 | rssi_data
int8 | rssi_beacon

The documentation for this struct was generated from the following file:

- .build.mcu/api-sources/thickmac/source/ti/drivers/net/wifi/wifi_host_driver/inc_adapt/wlan_if.h