# Smart PIR Motion Detection for CC1352

## Example Summary

The `smart_pir_detection_cc1352` example is designed for the CC13xx family of
devices and leverages [TI's Edge AI Studio](https://dev.ti.com/edgeaistudio/)
to enable the development of AI applications capable of efficiently running
locally on the device, on the Edge.

A Passive Infrared Sensor (PIR) is an electronic sensor that measures infrared
(IR) light radiating from objects in its direct field of view. These sensors are
commonly used as motion detectors in security alarms and automatic lighting
applications.

This example enhances traditional PIR-based motion detection by enabling
differentiation between targets based on their motion patterns. Using an AI Deep
Learning model, the system can classify motion types based on the PIR sensor's
analog signal.

[TI's Edge AI Studio](https://dev.ti.com/edgeaistudio/) guides users through
the entire AI pipeline process with these key steps:

1. Live Sensor Data Acquisition.
   Enables users to build application-specific datasets by acquiring data
   directly from sensors through the device. Users can label each dataset
   instance with the appropriate class and define the number of samples per
   instance and sampling frequency.

2. Model Selection.
   Allows users to select a pre-trained neural network architecture and suitable
   device for inference based on accuracy, speed, and cost considerations. The
   tool provides estimates of the model's footprint in terms of RAM, Flash
   usage, and inference time. For this example, the AI model (PIR-net) is
   pre-trained with a neural architecture proven to provide accurate results for
   this application.

3. Model Training.
   Enables selection of time and frequency-based features to be extracted from
   raw sensor data for training. Users can define training hyperparameters such
   as the number of epochs and learning rate. Feature extraction is supported on
   the MCU side through the feature extraction library.

4. Model Compilation.
   Compiles the trained AI model into efficient C code. The CC1352 uses a
   Cortex-M4F processor and the model is compiled targeting this architecture.

5. Live Inference Results Preview.
   Allows users to flash the complete application (including the compiled AI
   model) onto the device and run inference on real input sensor data with
   real-time result visualization. In this example, the AI model classifies
   motion as human, dog, or background.

## Edge AI Studio

[TI's Edge AI Studio](https://dev.ti.com/edgeaistudio/) is a collection of tools
that provide a fully integrated graphical user interface solution for collecting
and annotating data, training and compiling models for deployment on live
development platforms. Users can select from a variety of pre-trained models in
the TI Model Zoo and optionally re-train them with custom data to improve
accuracy and performance.

TI's Edge AI Studio is available as a cloud-based application for processor
devices and as both cloud and desktop applications for microcontrollers. When
using a microcontroller, the output from TI's Edge AI Studio is consumed by the
Code Composer Studio development environment.

## Prerequisites

Please go through the Release Notes to make sure you consider all the correct
hardware and software dependencies.

## Project Structure

1. ai_artifacts
    * Contains the AI neural network model header file `tvmgen_default.h` and
      pre-compiled source code `mod.a` that includes the model structure of the
      PIR-net. These files will be regenerated each time the user trains a new
      model through TI's Edge AI Studio.
    * These files can also be manually modified inside Code Composer Studio by
      compiling the model directly using [TI Neural Network Compiler for
      MCUs](https://software-dl.ti.com/mctools/nnc/mcu/users_guide/installing.html).
2. feature_extraction
    * `FeatureExtract_config`: Function to initialize FeatureExtract_Params
      based on a Model type; configured with default settings for the PIR-net
      neural network.
    * `FeatureExtract_run`: Function that executes a sequence of Feature
      Extraction functions for a specific model type. The following signal
      processing functions are enabled in the default sequence for PIR
      detection:
        * Windowing Function: Splits the input signal frame into multiple
          windows with an overlapping stride.
        * Fast Fourier Transform (FFT): Applies Real FFT with FP32 precision,
          where the number of bins depends on the sample length of each window.
        * Spectral Entropy: Calculates the randomness within a signal and
          determines the energy spread across the frequency distribution.
        * Zero Crossing Rate: Measures how often a signal crosses the zero axis,
          indicating the frequency or noisiness of a signal.
        * Changes in Slopes: measures the sign changes of signal differences.
        * Dominant Frequency: Determines the frequency components with the
          highest energy based on the energy distribution in the spectrum.
        * Temporal Kurtosis: Measures the impulsive nature of signal over time,
          indicating the presence of sharp motion events or outliers.
    *  `FeatureExtract_findClass`: Function to determine the appropriate labeled
       class/motion source based on the inferencing result of the PIR-net model.
3. sensor
    * `Sensor_init`: Function to initialize the Sensor Task that handles the
      configuration of the ADC and Timer drivers to start and stop data
      gathering based on the sampling frequency requested by TI's Edge AI
      Studio.
    * `Sensor_getData`: Function to start data sampling and transmit back the
      buffered sensor data to the main application task.
4. smart_detection_pir
    * Main application task that processes input from TI's Edge AI Studio
      through the Device Agent Protocol (DAP) to operate in different modes.
      Currently supported modes include:
        * Live preview of raw sensor data acquisition.
        * Live preview of sensor inferencing.
    * The Device Agent Protocol (DAP) is a UART-based serial communication
      protocol that enables the interaction between TI's Edge AI Studio (the
      host) and supported devices, specifically designed to work with TI's Edge
      AI Studio.

## Peripherals & Pin Assignments

When this project is built, the SysConfig tool will generate the TI-Driver
configurations into the __ti_drivers_config.c__ and __ti_drivers_config.h__
files and the TI-EdgeAI configuration into the __ti_edgeai_config.c__,
__ti_edgeai_config.h__ and __ti_edgeai_fe_config.h__ files. Information on
peripheral configuration, resources and parameters used is present in the
generated files. Additionally, the System Configuration file (\*.syscfg) present
in the project may be opened with SysConfig's graphical user interface to
determine the resources used.

* `CONFIG_ADC_0` - ADC instance.
* `CONFIG_TIMER_0` - Timer instance.

## BoosterPacks, Board Resources & Jumper Settings

For board specific jumper settings, resources and BoosterPack modifications,
refer to the __Board.html__ file.

* The BoosterPack that will be used in the Plugin is the **Edge AI Sensor
BoosterPack (TIDA-010997)**

## Example Usage

1. Connect the BoosterPack on top of the Launchpad.
    * This will connect the ADC channel defined in SysConfig to the PIR sensor
      sampling source.
    * __Note:__ Undefined values may be returned if the channel is not connected
      to a sampling source.

>__Important:__ Caution should be used when connecting the pins to analog inputs
greater than 3VDC.

2. Connect the Launchpad to the XDS110 debug probe.

3. Connect the XDS110 debug probe to the PC over USB.

The connection will have the following settings by default:

```text
    Baud-rate:     115200
    Data bits:          8
    Stop bits:          1
    Parity:          None
    Flow Control:    None
```

4. Go to [TI's Edge AI Studio](https://dev.ti.com/edgeaistudio/).

5. Select the Serial Port. Use the default baudrate (bps).

6. Now you are ready to follow the steps defined by [TI's Edge AI
   Studio](https://dev.ti.com/edgeaistudio/).
