EDGEAI API

Data Fields
DAP_Handle Struct Reference

DAP configuration. More...

`#include <ti/ai/edge_ai/dap/DAP.h>`

Collaboration diagram for DAP_Handle:

## Data Fields
UART2_Handle | uartHandle
MessageQueueP_Handle | messageQueueHandle
bool | isCrc
bool | startStreamingFlag
DAP_PipelineConfiguration | pipelineConfig

## Detailed Description

DAP configuration.

The DAP_Handle structure contains a set of pointers used to characterize the DAP implementation.

## Field Documentation

## § uartHandle

UART2_Handle DAP_Handle::uartHandle

UART handle

## § messageQueueHandle

MessageQueueP_Handle DAP_Handle::messageQueueHandle

Message Queue handle

## § isCrc

bool DAP_Handle::isCrc

## § startStreamingFlag

bool DAP_Handle::startStreamingFlag

## § pipelineConfig

DAP_PipelineConfiguration DAP_Handle::pipelineConfig

The documentation for this struct was generated from the following file:

- ti/ai/edge_ai/dap/DAP.h

© Copyright 1995-2026, Texas Instruments Incorporated. All rights reserved.
Trademarks | Privacy policy | Terms of use | Terms of sale