DMD, DMD Mounting, and Socket/Interposer Information Updated: 15 October 2025

Mounting Concept for Serie 600 DMD
This mounting information provides a reference concept for mounting DLP780NE, DLP781NE,DLP780TE, DLP781TE, DLP800RE, DLP801RE, DLP800XE, DLP801XE, DLP6500,DLP650NE, and DLP670RE DMDs. The DLP780NE, DLP780TE, DLP781NE, and DLP781TE utilize a FYU package, DLP800RE, DLP801RE, DLP800XE,and DLP801XE utilize a FYV package, and DLP6500, and DLP650NE utilize a FYE package. This mounting concept is for all Series 600 DMDs. Information includes: DMD 3D-CAD geometry model (STEP format) Link to DMD mechanical drawing - located at end of DMD data sheet Link to DMD data sheet (contains information like) Mounting and thermal load specifications Thermal specifications Array temperature calculation Electrical interconnect - mating connector information along with suppliers known at time of publishing Mechanical mounting concepts - has drawings (pdf format) and 3D-CAD geometry model (STEP format) for parts and assembly Getting Started Easy access to the files is provided with a web browser interface. Use of the web interface requires the files be downloaded and extracted to the computer. To utilize the web interface: Open the file 'READ-ME-s600-Mounting.htm' (this file) 'Right Click' on the downloaded file name and select ' Extract All...' (Note: Picking the file name will open the file but not extract the files) Select a destination to extract the files and select 'Extract' After extracting pick this link REVIEW_START-Series600.html or image below to start review (If the above link does not open the file or an image does not display below repeat Step (1) to extract the files)