DLP® DMD Mechanical, Thermal, Mounting, and Mating Connector Information Updated: 14 October 2025

Series 600 DMDs
(Select links in table below for detailed information)
DMD Information
DMD | Document | Document Number | Document Revision | Quantity I/O
DLP780NE .78 1080p HEP 1920 x 1080 | DMD Mechanical ICD - FYU package 3D CAD Geometry Model (STEP format) | 2516985 | C | 350 pins
DMD Data Sheet Internet access to TI.com is required for this link | DLP780NE | web
DLP781NE .78 1080p HEP 1920 x 1080 | DMD Mechanical ICD - FYU package 3D CAD Geometry Model (STEP format) | 2516985 | C
DMD Data Sheet Internet access to TI.com is required for this link | DLP781NE | web
DLP780TE .78 4K UHD HEP Displays 3840 x 2160 (1920 x 1080 native) | DMD Mechanical ICD - FYU package 3D CAD Geometry Model (STEP format) | 2516985 | C
DMD Data Sheet Internet access to TI.com is required for this link | DLP780TE | web
DLP781TE .78 4K UHD HEP Displays 3840 x 2160 (1920 x 1080 native) | DMD Mechanical ICD - FYU package 3D CAD Geometry Model (STEP format) | 2516985 | C
DMD Data Sheet Internet access to TI.com is required for this link | DLP781TE | web
DLP800RE .8 WUXGA HEP 1920 x 1200 | DMD Mechanical ICD - FYV package 3D CAD Geometry Model (STEP format) | 2517029 | A
DMD Data Sheet Internet access to TI.com is required for this link | DLP800RE | web
DLP801RE .8 WUXGA HEP 1920 x 1200 | DMD Mechanical ICD - FYV package 3D CAD Geometry Model (STEP format) | 2517029 | A
DMD Data Sheet Internet access to TI.com is required for this link | DLP801RE | web
DLP800XE .8 4K+ HEP Displays 3840 x 2400 (1920 x 1200 native) | DMD Mechanical ICD - FYV package 3D CAD Geometry Model (STEP format) | 2517029 | A
DMD Data Sheet Internet access to TI.com is required for this link | DLP800XE | web
DLP801XE .8 4K+ HEP Displays 3840 x 2400 (1920 x 1200 native) | DMD Mechanical ICD - FYV package 3D CAD Geometry Model (STEP format) | 2517029 | A
DMD Data Sheet Internet access to TI.com is required for this link | DLP801XE | web
DLP6500 .65 1080p 1920 x 1080 | DMD Mechanical ICD - FYE package 3D CAD Geometry Model (STEP format) | 2511543 | E
DMD Data Sheet Internet access to TI.com is required for this link | DLP6500 | web
DLP650NE .65 1080p 1920 x 1080 | DMD Mechanical ICD - FYE package 3D CAD Geometry Model (STEP format) | 2511543 | E
DMD Data Sheet Internet access to TI.com is required for this link | DLP650NE | web
DLP670RE .67 WUXGA HB 1920 x 1200 | DMD Mechanical ICD 3D CAD Geometry Model (STEP format) | 2513710 | B
DMD Data Sheet Internet access to TI.com is required for this link | DLP670RE | web
Mounting and Electrical Socket Information
For all Series 600 DMDs | DMD Mechanical Mounting Concepts PC Board Features (see specific concept) | Link |  |
Electrical Socket - 1.27 mm pitch 350 Contacts Socket, Zero Insertion Force Style 3D CAD Geometry Model (STEP format) Socket Supplier Information NOTE: The PCB pads for ZIF style socket are not inline (concentric) with pins on DMD. The PCB pads are shifted in one axis by 0.3875mm, see ZIF socket drawing. | 2511569 | A

Socket Supplier Information
Foxconn Interconnect Technology (FIT) ZIF Style Part Number: PZ35021-2641-01H List of parts for DMDs: Link If a list of DLP specific parts does not result select Search in upper right and use 'dlp' for search criteria. URL: https://www.fit-foxconn.com Contact Information: Use 'Online Contact Form' or 'Global Information' from URL Link NOTE: Texas Instruments has not qualified, or approved any specific parts or manufactures.