DLPC44XX GUI #VERSION#

Installation Location

The default installation directory is

C:\Program Files (x86)\DLPC44XX GUI #VERSION#

To install in a different directory, click the Browse button on the Select Features page.

DLPC44XX Controller Interface Drivers

When using DLPC44XX GUI, you must have a communications link established between the DLPC44XX controller and a computer running this software. This allows you to read and write to the controller from the computer. 

User needs to install device drivers using the DLP Driver Package.

Getting Help

Refer User_Guide_DLPC44XX.pdf to get help in using DLPC44XX GUI.