# SimpleLink™ SDK Edge AI Plugin 1.00.00.00 Release Notes

## Table of Contents

## Introduction

The SimpleLink™ SDK EdgeAI Plugin (EDGEAI) from Texas Instruments is a plugin for enabling EdgeAI development on TI’s Wireless MCUs leveraging the TI’s Edge AIs Studio.

## Documentation

The following documentation is provided with this release.

- Documentation Overview
- Software License
- Software Manifest

## What’s New

In this release of the Plugin, the following device support have been added to Smart PIR Motion Detection Example:

- CC1352R
- CC1352P7
- CC1354R10
- CC1354P10
- CC3551E

The plug-in contains the following features that have been developed:

- Device Agent Protocol (DAP).
- Feature Extraction Library.
- Support for Neural Processing Unit - Custom Datapath Extension (CDE).
- Smart PIR Motion Detection example.

## Fixed Issues

No bug fixes or known issues addressed in this release.

## Known Issues and Limitations

- Compiler support is currently limited to TI Clang.
- The PIR sensor example and the pre-trained PIR-net model in TI’s Edge AIs Studio expects a specific matrix of features as input. Therefore, the supported Feature Extraction library is not configurable in terms of features and their parameters. This will be modified in the future to enable flexibility while doing Model Training.
- The PIR sensor example and the pre-trained PIR-net model in TI’s Edge AIs Studio supports sampling frequencies between 25 and 50 Hz.
- The PIR sensor example and the pre-trained PIR-net model in TI’s Edge AIs Studio supports a fixed buffer of 125 bytes as input.
- For the following devices, a manual update needs to be done, wherein the ai_artifacts need to copied from the base example and copied over to the intended device example.

Device Example | Base Example
--- | ---
CC2755P10 | CC2745R10_Q1
CC1352P7 | CC1352R1
CC1354P10-6 | CC1354P10-1

## Operating System Support

- This Plugin supports only the same Operating System as the main SDK.

## Dependencies

EDGEAI requires the following dependency versions (or compatible):

- SimpleLink™ Low Power F3 SDK 9.12.00.19
- SimpleLink™ Low Power F2 SDK 8.31.00.11
- SimpleLink™ Wi-Fi SDK 9.21.00.15
- TI Clang 4.0.2.LTS-0
- Python 3.10.12
- TI’s Edge AIs Studio - Cloud Base
- TI’s Edge AIs Studio - Desktop Base EDGE-AI-STUDIO_1.6.0
- TI Sysconfig SysConfig 1.26.1.4441
- TI Neural Network Compiler for MCUs MCU_2.1.1 LTS

## Device Support

This SDK supports the following SimpleLink™ wireless MCUs:

Device | Orderable Part Number (OPN) | LaunchPad | Product Page | Migrate from these examples | SDK Dependency
--- | --- | --- | --- | --- | ---
CC2755R10 | CC2755R105E0WRHAR | LP-EM-CC2745R10-Q1 | CC2755R10 | LP-EM-CC2745R10-Q1 | SIMPLELINK-LOWPOWER-F3-SDK
CC2755P10 | CC2755P105E0WRHA | N/A | CC2755P10 | N/A | SIMPLELINK-LOWPOWER-F3-SDK
CC2745R10-Q1 | CC2745R10E0WRHARQ1 | LP-EM-CC2745R10-Q1 | CC2745R10-Q1 | LP-EM-CC2745R10-Q1 | SIMPLELINK-LOWPOWER-F3-SDK
CC2745R10-Q1 | CC2745R10E1WRHARQ1 | LP-EM-CC2745R10-Q1 | CC2745R10-Q1 | LP-EM-CC2745R10-Q1 | SIMPLELINK-LOWPOWER-F3-SDK
CC1352P7 | CC1352P74T0RGZR | LP-CC1352P7 | CC1352P7 | N/A | SIMPLELINK-LOWPOWER-F2-SDK
CC1352R | CC1352R1F3RGZ | LAUNCHXL-CC1352R1 | CC1352R | N/A | SIMPLELINK-LOWPOWER-F2-SDK
CC1354P10-6 | CC1354P106T0RGZ | LP-EM-CC1354P10 | CC1354P10-6 | N/A | SIMPLELINK-LOWPOWER-F2-SDK
CC1354P10-1 | CC1354P106T0RGZ | LP-EM-CC1354P10 | CC1354P10-1 | N/A | SIMPLELINK-LOWPOWER-F2-SDK
CC3551E | CC3550ENJARSHR | LP-EM-CC35X1 | CC3551E | N/A | SIMPLELINK-WIFI-SDK

## Versioning

All releases have 4 segment versions (M.mm.pp.bb). This includes GA and pre-releases (engineering, alpha/EA, beta, etc.). Pre-releases are denoted with a suffix (e.g. 1.00.00.00_eng).

This product’s version follows a version format, M.mm.pp.bb, where M is a single digit Major number, mm is 2 digit minor number, pp is a 2 digit patch number, and bb is an unrestricted set of digits used as an incrementing build counter.

To support multiple side-by-side installations of the product, the product version is encoded in the top level directory.

Subsequent releases of patch upgrades will be identified by the patch number. Typically, these patches only include critical bug fixes.

## Technical Support

- For support related to cc27XX devices please go to TI E2E BLE Connectivity Support Community
- For support related to cc135xxx devices please go to TI E2E sub-1 GHz Connectivity Support Community
- For support related to cc355xx devices please go to TI E2E Wi-Fi Connectivity Support Community

Last updated: 2026-03-04